This attribute identifies layer at which the switch has occurred. This layerRate can be used to filter the switch notification based on the layerRate.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
