Granularity granularity = NA, in Class TCAParameter

Documentation
This attribute defines the granularity of the TCAParameter.
For counters two values "15min" or "24h" are supported. For current instantaneous measurements
the granularity does not apply which is indicated by the value "NA".
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No