Specifies a list of cross-connects that must be used by the SNC. The list must be empty if no cross-connect constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.
