Contains the state of consistency between a TP and its associated egress TransmissionDescriptor.

Changes in the value of this attribute lead to a StateChange notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
