This attribute indicates the assignment of an ASAP to the TL.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? Only via assignASAP/deassignASAP operations.
Invariant? No
