The operation returns the capabilities of the EMS with information whether they are supported or not supported by the EMS (including the connection management modes indicating whether CC sharing, pending SNCs, and termination inclusion are supported; see attached supporting document modesOfOperation for explanation).

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
