Indicates if the reroute (if allowed) should be computed by the network (Yes), by the EMS (No), or if it does not matter (Not_Set).

Changes in the value of this attribute shall lead to an AVC notification.

Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes
