Identifies a unidirectional measurement provided by a source monitoring function of this TP. The opposite direction of the supervised signal is measured.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
