tmf854.v1 > HoldOffTime_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The HoldOffTime_T Simple Type
This is the time duration for which the alarm condition must persist before the switch takes place. Values are in milliseconds.
<ApplicableTo> All protection groups that support revertive switch. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type HoldOffTime_T
HoldOffTime_T is union of (string, unsignedLong).
• string: There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (Unknown | Infinite).

Enumeration | Description
Unknown |
Infinite |

• unsignedLong: There are several restrictions on the value. The range of the value is [0..18446744073709551615]. The schema processor collapses value's whitespace. The number of fractional digits is less than or equals to 0.

XML
-<xsd:simpleType name="HoldOffTime_T"> -<xsd:annotation> -<xsd:documentation> This is the time duration for which the alarm condition must persist before the switch takes place. Values are in milliseconds. <ApplicableTo> All protection groups that support revertive switch. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:union> -<xsd:simpleType> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="Unknown" /> <xsd:enumeration value="Infinite" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> <xsd:restriction base="xsd:unsignedLong"> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType>

﻿

Uses
Type (2) string unsignedLong

Used-By
Element (1) PGPParameters_T/HoldOffTime

Generated by WSDLdoc ©