Provides an indication of whether alarm reporting for this subnetwork connection is administratively activated or de-activated.
Changes in the value of this attribute lead to a AVC notification.

True = alarm reporting is activated; False = alarm reporting is de-activated.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
