Integer EVENT_ACKNOWLEDGED = 1, in Class AcknowledgeIndication

Documentation
Used in case that the alarm has been acknowledged in the EMS. All alarm fields other than emsTime and acknowledge indication shall remain similar to the original alarm notification.
(The emsTime is always provided as the time that the alarm acknowledgement notification has been reported by the EMS.)
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No