Operation void getAllSupportingEquipmentNames (CIS SequenceOf Name equipmentNames = NA), in Class PhysicalTerminationPoint

Documentation
This operation implements the 'supporting' relationship (see equipment model) between PTPs and circuit pack.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS dos not supported this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

equipmentNames
/* out */ The name(s) of the equipment directly implementing this PTP.