Specifies a list of PTPs and/or CTPs that must be used by the SNC. The list must be empty if no PTP/CTP constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.

Note: In case of bundled SNCs,
- for each PTP used in the inclusion list, the EMS should use a GTP that contains at least one CTP from the given PTP
- for each CTP used in the inclusion list, the EMS should use a GTP that contains the given CTP.
