CIS SequenceOf Structs::AVP additionalCreationInfo = empty list, in Class SNCCreateData

Documentation
Some additional information may be specified by the NMS. For example:
- for a system which cannot use the routing constraints for a BLSR case it may supply the pairs:
- "BLSRDirection" taking values "EAST", "WEST" and "NA"
- "Timeslot" taking values "1".."nnnnn".
- this could also be used to carry the "PotentialFutureSetupIndicator" of the aEnd in the case where it has an impact on the creation of the SNC for unidirectional point-to-multipoint configurations.
The list may be empty.
Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No