Specifies a list of TopologicalLinks that must be used by the SNC. The list must be empty if no TopologicalLink constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.
