tmf854.v1 > ProbableCause_T LOCATION: file:/xsd/networkResources/ProbableCauses.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ProbableCause_T Complex Type
The MTOSI alarm probable causes. For details refer to the supporting document: ProbableCauses.

Local elements (3)
  ru contra type

Complex Type ProbableCause_T
The ProbableCause_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... overlap="xsd:string" qualifier="xsd:string"> -Begin All [1...1] This boolean parameter stands for Remote Unit (RU). It indicates the location of the network resource the alarm probable cause is associated with. The default setting (false) is for an alarm detected with a local network resource. And, the value is "true" when the alarm is associated with a remote network resource. <ru>xsd:boolean</ru> [0..1] This is a boolean parameter used to distinguish the direction of the signal related alarm. The default setting (false) is for an alarm detected on the signal that is related to the sink atomic function. And, the value is "true" for an alarm detected on the signal that is related to the source atomic function. <contra>xsd:boolean</contra> [0..1] This is the probable cause specific value. <type>union of (string, string, string, string)See XML snippet for more information.</type> [1..1] End All </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
overlap | string | This attribute is optional. Its form is unqualified. Show details.
Base type of overlap is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
qualifier | string | This attribute is optional. Its form is unqualified. Show details.
Base type of qualifier is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:complexType name="ProbableCause_T"> -<xsd:annotation> <xsd:documentation> The MTOSI alarm probable causes. For details refer to the supporting document: ProbableCauses. </xsd:documentation> </xsd:annotation> -<xsd:all> -<xsd:element default="false" minOccurs="0" name="ru" type="xsd:boolean"> -<xsd:annotation> <xsd:documentation> This boolean parameter stands for Remote Unit (RU). It indicates the location of the network resource the alarm probable cause is associated with. The default setting (false) is for an alarm detected with a local network resource. And, the value is "true" when the alarm is associated with a remote network resource. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element default="false" minOccurs="0" name="contra" type="xsd:boolean"> -<xsd:annotation> <xsd:documentation> This is a boolean parameter used to distinguish the direction of the signal related alarm. The default setting (false) is for an alarm detected on the signal that is related to the sink atomic function. And, the value is "true" for an alarm detected on the signal that is related to the source atomic function. </xsd:documentation> </xsd:annotation> </xsd:element> -<xsd:element name="type"> -<xsd:annotation> <xsd:documentation> This is the probable cause specific value. </xsd:documentation> </xsd:annotation> -<xsd:simpleType> -<xsd:union> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI extensions in a minor version. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="MINOR_([a-z]|[A-Z]|[0-9]|(_-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the vendor specific extensions must start with the prefix "PROP_" </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="PROP_([a-z]|[A-Z]|[0-9]|(_-))*" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI pre-defined probable causes. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="UNIDENTIFIED" /> <xsd:enumeration value="AIS" /> <xsd:enumeration value="AMS" /> <xsd:enumeration value="ATPC_FAIL" /> <xsd:enumeration value="AU-AIS" /> <xsd:enumeration value="BER_SD" /> <xsd:enumeration value="BER_SF" /> <xsd:enumeration value="BLOCKED_FE" /> <xsd:enumeration value="CFG_ABORT" /> <xsd:enumeration value="CFG_ABORT_FE" /> <xsd:enumeration value="DCC_FAILURE" /> <xsd:enumeration value="DEMODULATION_FAIL" /> <xsd:enumeration value="EMS" /> <xsd:enumeration value="EMS_ALM_LOSS" /> <xsd:enumeration value="EMS_LIFECYCLE_LOSS" /> <xsd:enumeration value="EMS_ALM_AND_LIFECYCLE_LOSS" /> <xsd:enumeration value="EQPT" /> <xsd:enumeration value="ENV" /> <xsd:enumeration value="FF" /> <xsd:enumeration value="FOP_APS" /> <xsd:enumeration value="INSUFF_LINKS" /> <xsd:enumeration value="INSUFF_LINKS_FE" /> <xsd:enumeration value="LCD" /> <xsd:enumeration value="LIF" /> <xsd:enumeration value="LOA" /> <xsd:enumeration value="LOC" /> <xsd:enumeration value="LODS" /> <xsd:enumeration value="LOF" /> <xsd:enumeration value="LOM" /> <xsd:enumeration value="LOP" /> <xsd:enumeration value="LOPC" /> <xsd:enumeration value="LOS" /> <xsd:enumeration value="LOTC" /> <xsd:enumeration value="MODULATION_FAIL" /> <xsd:enumeration value="MS-AIS" /> <xsd:enumeration value="OS" /> <xsd:enumeration value="OS_ALM_LOSS" /> <xsd:enumeration value="OS_LIFECYCLE_LOSS" /> <xsd:enumeration value="OS_ALM_AND_LIFECYCLE_LOSS" /> <xsd:enumeration value="OSC-AIS" /> <xsd:enumeration value="OSC_BER_SF" /> <xsd:enumeration value="OSC_FERF" /> <xsd:enumeration value="OSC_LOF" /> <xsd:enumeration value="OSC_LOS" /> <xsd:enumeration value="OSC_SD" /> <xsd:enumeration value="PLM" /> <xsd:enumeration value="RAI" /> <xsd:enumeration value="RX_FAIL" /> <xsd:enumeration value="RX_MIS_CONNECT" /> <xsd:enumeration value="RX_UNUSABLE_FE" /> <xsd:enumeration value="SECURITY_VIOLATION" /> <xsd:enumeration value="SQL" /> <xsd:enumeration value="SSF" /> <xsd:enumeration value="STARTUP_FE" /> <xsd:enumeration value="TCF" /> <xsd:enumeration value="TCFE" /> <xsd:enumeration value="TCFI" /> <xsd:enumeration value="TIM" /> <xsd:enumeration value="TIMING_SYNCH" /> <xsd:enumeration value="TSD" /> <xsd:enumeration value="TSF" /> <xsd:enumeration value="TU-AIS" /> <xsd:enumeration value="TX_DEGRADE" /> <xsd:enumeration value="TX_FAIL" /> <xsd:enumeration value="TX_MIS_CONNECT" /> <xsd:enumeration value="TX_UNUSABLE_FE" /> <xsd:enumeration value="UAT" /> <xsd:enumeration value="UNEQ" /> <xsd:enumeration value="VC-AIS" /> <xsd:enumeration value="VC-RDI" /> <xsd:enumeration value="VP-AIS" /> <xsd:enumeration value="VP-RDI" /> <xsd:enumeration value="XPIC_FAIL" /> </xsd:restriction> </xsd:simpleType> -<xsd:simpleType> -<xsd:annotation> <xsd:documentation> All the MTOSI pre-defined specific TCM probable causes. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:pattern value="TCM(_(AIS|LOS|OAI|RAI|SD|SSF|TIM|UNEQ|(LEVEL[1-6]_(LCK|LOS|OCI|RAI|SD|SSF|TIM))))?" /> </xsd:restriction> </xsd:simpleType> </xsd:union> </xsd:simpleType> </xsd:element> </xsd:all> <xsd:attribute name="overlap" type="xsd:string" use="optional" /> <xsd:attribute name="qualifier" type="xsd:string" use="optional" /> </xsd:complexType>

﻿

Uses
Type (2) boolean string

Used-By
Element (2) Alarm_T/probableCause ProbableCauseList_T/probableCause

Generated by WSDLdoc ©