This operation implements the 'supports' relationship (see equipment model) between equipment and PTPs for the NMS.This operation returns an empty list for a protecting card.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS- Raised when communication to managed element is lost.
