The attribute defines the priority of the SNC.
Allowed values are = "0" , "1" , "2" , ... where zero (0) is the highest priority.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
