Operation void createTransmissionDescriptor (TransmissionDescriptorCreateData transmissionDescriptorCreateData = NA, TransmissionDescriptor newTD = NA), in Class EMS

Documentation
The operation creates a new TransmissionDescriptor.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when transmissionDescriptorCreateData contains invalid data.
4. USERLABEL_IN_USE - Raised when the userLabel uniqueness constraint is not met.
5. CAPACITY_EXCEEDED - Raised when maximum number of Transmission Descriptors has been reached.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Requested TransmissionDescriptor exists.
Semantics

Arguments

transmissionDescriptorCreateData
/* in */ The data that describes the TransmissionDescriptor to be created.
newTD
/* out */ The distinguishing information of the created TransmissionDescriptor.