CIS CharacterString X.733::EventType = Absent from notification, in Class AlarmInformation

Documentation
The optional Event Type parameter, when present in an alarm notification, classifies the alarm into one of the five basic categories specified in ITU-T X.733.
This is consistent with the ITU-T X.733 definition.
Value is one of the following:
- "communicationsAlarm",
- "environmentalAlarm",
- "equipmentAlarm",
- "processingErrorAlarm",
- "qualityOfServiceAlarm"
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No