tmf854.v1 > ProtectionGroup_T > G_774_3_APSfunction
LOCATION: file:/xsd/networkResources/Protection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The G_774_3_APSfunction Element
Indicates if the switching function is based on APS standardized protocol or on a proprietary protocol. "G.783" is set in case of K1/K2 based APS, and "Legacy" is set in case of proprietary protocol, as for radio equipment for example (values "G.783", "Legacy")
Element ProtectionGroup_T/G_774_3_APSfunction : G_774_3_APSfunction_T [0 .. 1]
The G_774_3_APSfunction element can have "xsi:nil" as an attribute. The G_774_3_APSfunction element in XML instance can be substituted with other elements.

XML Instance
Indicates if the switching function is based on APS standardized protocol or on a proprietary protocol. "G.783" is set in case of K1/K2 based APS, and "Legacy" is set in case of proprietary protocol, as for radio equipment for example (values "G.783", "Legacy") <G_774_3_APSfunction>G_774_3_APSfunction_T</G_774_3_APSfunction>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="G_774_3_APSfunction" nillable="true" type="G_774_3_APSfunction_T"> -<xsd:annotation> <xsd:documentation> Indicates if the switching function is based on APS standardized protocol or on a proprietary protocol. "G.783" is set in case of K1/K2 based APS, and "Legacy" is set in case of proprietary protocol, as for radio equipment for example (values "G.783", "Legacy") </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) G_774_3_APSfunction_T

Used-By

Generated by WSDLdoc ©