CIS SequenceOf Structs::AVP additionalObjectInformation = empty list, in Class TransmissionDescriptor

Documentation
The attribute contains additional info parameters which can be set and/or retrieved on an object having this TransmissionDescriptor (TMD) assigned as egress or ingress TMD.
Changes in the value of this attribute lead to an AVC notification.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No