This attribute specifies if the route for this SNC is computed by the network.
If rerouting is allowed, this attribute tells who last rerouted the SNC, the network (YES) or the EMS (NO).

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
