This operation retrieves the ASAP(s) which are assigned to the addressed resource. The ASAP list can have zero or more elements, as all resources but TPs can refer to at most one ASAP. TPs can refer to more ASAPs, at most as many as the number of encapsulated layer rates.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when layerRateList is invalid for the addressed resource, i.e. it is not an encapsulated
    layerRate.
4. ENTITY_NOT_FOUND - Raised when resourceName references an object that does not exist.
5. UNABLE_TO_COMPLY - Raised in case resourceName refers to an object not supporting the ASAP pointer feature.
