Operation void getAllEquipment (CIS SequenceOf of Choice objects), in Class EquipmentHolder

Documentation
This allows an NMS to request all of the equipment and equipment holders that are contained in this equipment holder.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Equipment or EquipmentHolder objects returned.
Semantics

Arguments

objects
/* out */ List of Equipment and/or Equipment Holders (with complete object information).