Operation void getHoldingTime (HoldingTime holdingTime = NA), in Class PerformanceManager

Documentation
This operation allows the NMS to know how many hours PM data records are held in the EMS (worst case time).
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

holdingTime
/* out */ Gives the worst case time an EMS can hold PM data for 15 min and 24h Data.