Operation void setTCAParameterProfilePointer (Name addTCAParameterProfile = CIS Null, Name removeTCAParameterProfile = CIS Null), in Class TerminationPoint

Documentation
This operation adds/removes TCA Parameter Profiles to/from the TP.
The new threshold values contained in the added profiles will be copied to the corresponding PMPs of the TP.
The addition of an already associated profile to a TP overwrites the corresponding thresholds
in the PMPs of the TP.
The threshold values that have been configured via a profile to be removed will be kept in the PMPs.
Note: No further automatic updating based on changes in the profile will be done.
See corresponding activity diagram.
Note: This operation can also be used to align the TCA Thresholds of all PMPs
contained in the TP with the threshold values contained in the associated TCA
Parameter Profile and is therefore idempotent.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when TCA Parameter Profile to be assigned does not exist.
5. OBJECT_IN_USE - Raised when TCAParameterProfile of same Layer is already assigned to the TP.
6. UNABLE_TO_COMPLY - Raised when threshold values in the TP could not be configured.
7. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
TCA Parameter Profile specified must exist.
Postconditions
The threshold values of the TP are consistent with the added/removed TCA Parameter Profiles.
Semantics

Arguments

addTCAParameterProfile
/* in */ The name of the TCAParameterProfile to be added to this TP.
removeTCAParameterProfile
/* in */ The name of the TCAParameterProfile to be removed from this TP.