CIS SequenceOf Structs::EndPointRole aEndPointsRole = NA, in Class SubnetworkConnection

Documentation
This attribute indicates the end point role of the aEndTPs of the SNC.
At a connection matrix (CM) end point the span of the SNC starts at a G.805 CP with a fixed or flexible connection through the ME at the SNC layer, i.e. the connectable layer of the end point. At a link connection (LC) end point connectivity is adapted from a server layer and the span of the SNC starts with a G.805 TCP.
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No