This structure represents one performance monitoring point including performance monitoring and threshold supervision. 
There always exists one PMP for every triple of layer rate, PM location and granularity for which the containing TP is capable to monitor performance.
Thus, its existence reflects the TP's PM capabilities.

Object Lifecycle: Created and deleted by EMS.

Object Creation Notification Issued? Yes
Object Deletion Notification Issued? Yes
