Operation void retrieveSwitchData (SwitchData switchData), in Class ConnectionTerminationPoint

Documentation
This operation is used by the NMS to get the latest switch status on a SNCP.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS is unable to support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
The Termination Point is in a protection configuration (SNCP).
Postconditions
The switch data is available to the NMS.
Semantics

Arguments

switchData
/* out */ Switch Data
In the returned switchData object the protectionType is fixed to SNCP and the group name is fixed to Null.