A TP pool (TPPool) represents a set of termination points or group termination points that are grouped (without a specific order) for some administrative management purpose such as bandwidth reservation or common routing. The TPs and GTPs of the TPPool must belong to the same Subnetwork.
A termination point that is a member of a GTP cannot be a member of a TPPool independent of the other CTPs in the GTP.
Properties that are common for all the TPs in the TPPool are identified in the multiple associated CommonTransmissionParameters objects.
Changes in the value of the contained Common Transmission Parameters lead to a AVC notification.

MTOSI Specific Documentation
This class is applicable to MTOSI. The specific operations and relationships that apply to MTOSI are listed in SD2-11. 
For MTOSI, references to "NMS" can be interpreted as "Requesting OS" and references to "EMS" can be interpreted as "Target OS", i.e., the OS that fulfills requests from another OS. 
The statements concerning Object Lifecycle, i.e., whether the object can be created by the NMS or EMS, are not particularly meaningful for MTOSI, since MTOSI does not define management systems with fixed roles such as the NMS and EMS entities in MTNM.

Object Lifecycle: Created and deleted by EMS or NMS.

Object Creation Notification Issued? Yes
Object Deletion Notification Issued? Yes
Object Discovery Notification Issued? Yes
