tmf854.v1 > ReversionMode_T LOCATION: file:/xsd/networkResources/Protection.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The ReversionMode_T Simple Type
Reversion mode is used to indicate whether, after repair of a failed resource, an additional switch should be made to revert to the preferred resource. Revertive modes may require a wait to restore (WTR) time setting.
Simple Type ReversionMode_T
ReversionMode_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (RM_UNKNOWN | RM_NON_REVERTIVE | RM_REVERTIVE).

Enumeration | Description
RM_UNKNOWN |
RM_NON_REVERTIVE |
RM_REVERTIVE |

XML
-<xsd:simpleType name="ReversionMode_T"> -<xsd:annotation> <xsd:documentation> Reversion mode is used to indicate whether, after repair of a failed resource, an additional switch should be made to revert to the preferred resource. Revertive modes may require a wait to restore (WTR) time setting. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="RM_UNKNOWN" /> <xsd:enumeration value="RM_NON_REVERTIVE" /> <xsd:enumeration value="RM_REVERTIVE" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (2) EProtectionGroup_T/reversionMode ProtectionGroup_T/reversionMode

Generated by WSDLdoc ©