tmf854.v1 > retrieveESwitchData_T LOCATION: file:/xsd/interfaces/ProtectionMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The retrieveESwitchData_T Complex Type
This service is used by the NMS to get the latest switch status on an equipment protection group. For a retrieval of a revertive M:N group, N ESwitchData_T are returned as a result of retrieveESwitchData (one for each worker equipment instance). For a retrieval of a non-revertive M:N group, N ESwitchData_T are returned as a result of retrieveESwitchData (one for each active equipment instance). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised when an OS is unable to support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when ePGPName does not reference an equipment object EXCPT_ENTITY_NOT_FOUND - Raised when ePGPName references object which does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost

Local elements (1)
  ePGPName

Complex Type retrieveESwitchData_T
The retrieveESwitchData_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> This is the equipment protection group name for which the switch data is being requested. <ePGPName extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</ePGPName> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="retrieveESwitchData_T"> -<xsd:annotation> <xsd:documentation> This service is used by the NMS to get the latest switch status on an equipment protection group. For a retrieval of a revertive M:N group, N ESwitchData_T are returned as a result of retrieveESwitchData (one for each worker equipment instance). For a retrieval of a non-revertive M:N group, N ESwitchData_T are returned as a result of retrieveESwitchData (one for each active equipment instance). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised when an OS is unable to support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised when ePGPName does not reference an equipment object EXCPT_ENTITY_NOT_FOUND - Raised when ePGPName references object which does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="ePGPName" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> This is the equipment protection group name for which the switch data is being requested. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) retrieveESwitchData

Generated by WSDLdoc ©