Operation void destroyGCT ( CIS CharacterString gCTDisplayAddress = NA), in Class EMS

Documentation
Closes all GCT opened by launchGCT() at the given GCTDisplayAddress
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised in case when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised in case input data is invalid.
4. ENTITY_NOT_FOUND - Raised when there are no GCT windows that are managed by the EMS open
at the given display host address.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
1. The EMS is able to manage GCT application windows.
2. The EMS has 1 or more GCT applications that have been launched directly by the EMS (under a "server launched" configuration) being displayed at the given GCTDisplayAddress.
Postconditions
1. All of the GCT windows opened by the EMS at the given display host address are closed.
2. The relevant GCT records maintained by the EMS are cleared.
Semantics

Arguments

gCTDisplayAddress
/* in */ The IP address or hostname including any display port information.