Defines if at least one of the routes XCs or CTPs is carrying traffic of another SNC (True).

Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
