ControlState supervisionState = Locked, in Class PerformanceMonitoringPoint

Documentation
The supervision state indicates whether performance threshold supervision is enabled or disabled for the PMP.
Changes in this attribute lead to a State Change notification.
Readable by NMS? Yes
Writeable by NMS? Via operations enableTCA() / disableTCA()
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No