This operation returns the EMS profiling information that applies to the GUI Cut-through: indication of support for the "server-launch", the supported GCT contexts and scopes, GCT command information necessary to launch the GCT on the client side.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
