Operation void getAllEquipmentNames (CIS SequenceOf Name objectNames), in Class EquipmentHolder

Documentation
This allows an NMS to request all of the names of equipment and equipment holders that are contained in this equipment holder.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
Equipment or Equipment Holder names returned.
Semantics

Arguments

objectNames
/* out */ List of equipment and/or equipment holder names.