Specifies a list of GTPs that must be used by the route. The list must be empty if no GTP constraints are required. If the EMS cannot fully satisfy the constraints, then the request will be rejected.
