Operation void getAllEMSAndMEActiveAlarms (CIS SequenceOf Strings::ProbableCause excludeProbCauseList = empty list, CIS SequenceOf Enums::PerceivedSeverity excludeSeverityList = empty list, CIS SequenceOf AlarmInformation activeAlarmList = empty list), in Class EMS

Documentation
This operation allows an NMS to request all of the active alarms and TCAs that are under the control of this EMS (both those raised by the NEs and those raised by the EMS itself).
Note: A raised alarm is called active as long as no clear notification was received.
Alarms which ASAP assigned severity is "NOT_ALARMED" should not be reported by this operation.
Operation Exceptions:
INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

excludeProbCauseList
/* in */ The list of probable causes to exclude (for which events should not be reported).
excludeSeverityList
/* in */ List of severities to exclude from the output event list.
activeAlarmList
/* out */ List of active alarm(s) or empty list.