tmf854.v1 > SubnetworkConnectionList_T > snc
LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The snc Element
Element SubnetworkConnectionList_T/snc : SubnetworkConnection_T [0 .. *]
The snc element cannot have "xsi:nil" as an attribute. The snc element in XML instance can be substituted with other elements.

XML Instance
<snc extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> -Begin All [1...1] This attribute represents a unique identifier for the object on the CCV. Refer to the type definition for more details. <name extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</name> [0..1] This attribute represents a unique identifier for the object when its existence is first published on the CCV. Refer to the type definition for more details. <discoveredName>DiscoveredName_T</discoveredName> [0..1] This attribute contains the name of the OS that provided the unique MTOSI name for the object. Refer to the type definition for more details. <namingOS>NamingOS_T</namingOS> [0..1] "User-friendly" name for the object. Refer to the type definition for more details. <userLabel>UserLabel_T</userLabel> [0..1] Indicates whether the object was discovered or entered in OS inventory. Refer to the type definition for more details. <source qualifier="xsd:string">Source_T</source> [0..1] Identifier for the owner of the object. Refer to the type definition for more details. <owner>Owner_T</owner> [0..1] List of aliases for the network entity. Refer to the type definition for more details. <aliasNameList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">AliasNameList_T</aliasNameList> [0..1] Indicates the state of the resource. Refer to the type definition for more details. <resourceState overlap="xsd:string" qualifier="xsd:string">ResourceState_T</resourceState> [0..1] The sncState is an attribute managed by the EMS. The EMS manages the state transition of this attribute. The EMS will assess the cross-connections in the network that support the SNC and will appropriately adjust the value of SNCState to reflect the actual state of the SNC in the network. <sncState>SNCState_T</sncState> [0..1] Specifies the direction of the subnetwork connection. <direction>ConnectionDirection_T</direction> [0..1] The rate of the SubnetworkConnection is obtained by reading this attribute. <rate>LayerRate_T</rate> [0..1] The static protection level of the SNC. For a detailed description of the use of this attribute, see SNC Types. <staticProtectionLevel>StaticProtectionLevel_T</staticProtectionLevel> [0..1] The type of the SNC. For a detailed description of the use of this attribute, see SNC Types. <sncType>SNCType_T</sncType> [0..1] The list of Aend termination points TP where this SNC terminates. For a detailed description of the use of this attribute, see MTNM SNC Types supporting document. <aEnd>TPDataList_T</aEnd> [1..1] The list of Zend termination points TP where this SNC terminates. For a detailed description of the use of this attribute, see MTNM SNC Types supporting document. <zEnd>TPDataList_T</zEnd> [1..1] This attribute indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC <rerouteAllowed>Reroute_T</rerouteAllowed> [0..1] This attribute specifies if the route for this SNC is computed by the network. <networkRouted>NetworkRouted_T</networkRouted> [0..1] A free-format string used to associate the resource to a Network Access Domain. <networkAccessDomain>NetworkAccessDomain_T</networkAccessDomain> [0..1] Provides an indication whether alarm reporting for this instance is active or not. <alarmReportingIndicator>xsd:boolean</alarmReportingIndicator> [0..1] Takes value True when all cross-connects of the SNC are fixed. <fixed>xsd:boolean</fixed> [0..1] Allows for additional information to be modeled <vendorExtensions extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">SNCVendorExtensions_T</vendorExtensions> [0..1] End All </snc>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
qualifier | string | This attribute is optional. Its form is unqualified. Show details.
Base type of qualifier is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
overlap | string | This attribute is optional. Its form is unqualified. Show details.
Base type of overlap is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
qualifier | string | This attribute is optional. Its form is unqualified. Show details.
Base type of qualifier is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
<xsd:element maxOccurs="unbounded" minOccurs="0" name="snc" type="SubnetworkConnection_T" />

﻿

Uses
Type (1) SubnetworkConnection_T

Used-By

Generated by WSDLdoc ©