tmf854.v1 > TransmissionDescriptor_T > transmissionParams
LOCATION: file:/xsd/networkResources/TransmissionDescriptor.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The transmissionParams Element
A list of transmission parameters which can be set and retrieved at a specified layer on a TP having this TMD assigned as egress or ingress TMD
Element TransmissionDescriptor_T/transmissionParams : LayeredParametersList_T [0 .. 1]
The transmissionParams element can have "xsi:nil" as an attribute. The transmissionParams element in XML instance can be substituted with other elements.

XML Instance
A list of transmission parameters which can be set and retrieved at a specified layer on a TP having this TMD assigned as egress or ingress TMD <transmissionParams> <layeredParameters extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">LayeredParameters_T</layeredParameters> [0..*] </transmissionParams>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element minOccurs="0" name="transmissionParams" nillable="true" type="LayeredParametersList_T"> -<xsd:annotation> <xsd:documentation> A list of transmission parameters which can be set and retrieved at a specified layer on a TP having this TMD assigned as egress or ingress TMD </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) LayeredParametersList_T

Used-By

Generated by WSDLdoc ©