A list of transmission parameters per layer rate which can be set and/or retrieved on the TP.
Note: Setting is prohibited for some specific parameters.
This object can be set by an NMS through the ME.setTPData() and also during SNC creation.

Object Lifecycle: Lifecycle tied to TP.

Object Creation Notification Issued? NA
Object Deletion Notification Issued? NA
