Operation void getAllFTPs (CIS SequenceOf Enums::LayerRate tpLayerRates = empty list, CIS SequenceOf Enums::LayerRate connectionLayerRates = empty list, CIS SequenceOf FloatingTerminationPoint ftps = NA), in Class ManagedElement

Documentation
Get a filtered set of the FTPs together with their associated distinguishing information that contain one or more of the NMS-specified TP layer rates and that are capable of containing CTPs that can be connected at one or more of the NMS-specified connection layer rates. This operation considers the capability/flexibility of the FTPs, not their current states.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when tpLayerRateList or connectionLayerRateList contain undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

tpLayerRates
/* in */ A list of TP Layer Rates used to scope the request. If the list is empty, all FTPs are returned
connectionLayerRates
/* in */ The set of connection layer rates from which the reported FTPs must support at least one. If the list is empty then all FTPs are returned.
ftps
/* out */ A list of FTPs that are capable of supporting the provided TP and connection layer rates.