Name switchAwayFromTP = NA, in Class ProtectionSwitch

Documentation
Identifies the TP being switched away from.
- In case of 2F MSSPRING, this is the TP that switched. The East and the WEST side can switch independently. This is one of the TPs that switched.
- In case of 4-Fiber rings, when a span switch occurs, this is one of the TPs in the MSP ( 1+1, 1:n) groups (worker or protection).
- In case of a ring switch, this is the worker TP of the span that switched. For example if the EAST span switches to the WEST span then this TP is the East - Worker.
- In case of SNCP, this is the TP that the traffic source switched away from.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No