Specifies whether uniqueness of the userLabel is required amongst ASAPs of the EMS.
The operation will fail if the provided userLabel is already in use.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
