CIS Boolean alarmReportingIndication = FALSE, in Class SNCCreateData

Documentation
Indicates whether alarm reporting for the subnetwork connection is administratively activated or de-activated.
True = alarm reporting is activated; False = alarm reporting is de-activated.
Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No