Get a set of TP Pools and their associated distinguishing information contained by this subnetwork.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised if the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
