This operation will abort a backup of ME configuration data that is pending or in progress. If there is no backup of configuration data of the ME pending or in progress an exception will be thrown.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when specified managed element does not exist.
5. NE_COMM_LOSS - Raised when communication to the ME is lost.
6. NOT_IN_VALID_STATE - Raised when there is no pending/in progress backup of configuration data on the
    specified managed element.
