This operation allows the NMS to request a filtered set (scoped by the input parameter pmParameters) current PM data for a list of TP measurement points.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does support only history/previous data.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when pmTPSelectList is empty or contains invalid data.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
